DER- luminaires / Stainless steel luminaire / FS 804

FS 804.1 WE LED 48 V IP65 - (100709743)

Dynamic emergency exit sign luminaire FS 804.1WE D.E.R. 48V  stainless steel

Dynamic escape route segment luminaire with run light function and high degree of protection made of stainless steel to indicate the safe escape route depending on the smoke spreading during a fire. Power supply via PSU 48. 

The following characteristics need to be complied with:

Zweikanaliger LED-Treiber mit integrierter Einzelleuchtenüberwachung. Hohe Funktionssicherheit durch Einhaltung internationaler Standards zur Sicherheit und Arbeitsweise, elektromagnetische Verträglichkeit und Störsicherheit. Zum Anschluss an INOTEC SEV oder SEV-A.

- Mounting type: recessed wall mounting
- Material: stainless steel
- Dim.: Length x Width x Height: 120 mm x 120 mm x 60 mm
- Input terminal: 1.5mm²

- Illuminant: 4 x 1W LED-module
- Service life: 50.000 h

- Protection category: IP65
- Protection class: III
- Rated voltage: 48 V DC +/-10 %
- Power consumption battery operation: 35 mA
- Permitted temperature range: -15...+40 °C

5-year manufacturer's warranty on INOTEC brand products.
10-years of resupply guarantee for compatible LED-modules and wear parts

Made in Germany

Version of the luminaire named above acc. to DIN VDE V 0108-100-1, IEC 60598-1, IEC 60598-2-22, DIN 4844 and EN 1838. EMC protection acc. To EN 550 15.

LED driver according to EN 61347-1, EN 61347 2-13 and EN 61547.

An CE declaration of conformity for compliance with the Low Voltage Directive 2014/35/EC, RoHS Directive 2011/65/EU, electromagnetic compatibility 2014/30/EU and the above-mentioned standards must be documented. In addition, data sheets must be provided for documentation purposes.

When a different brand is offered, the equality of the characteristics needs to be recorded in written form and added to the offer. A lighting calculation needs to be demonstrated and added to the offer for safety lightings. Additional costs that occur due to the different brand are not refundable.

Brand: INOTEC Sicherheitstechnik GmbH
or equivalent and ready for use.